iFLASH Release 2.0
 
This utility is used to save and update FLASH memory. It is recommended 
that this utility be executed from a bootable MS-DOS diskette that 
contains BIOS recovery files for the target system (i.e. BIOS.REC). 
 
This utility must be executed in a system without memory managers installed. 
If EMM386, QEMM, 386MAX, or Windows is active, then the FLASH update 
is not safe.  Remove any memory manager or exit Windows before executing 
the FLASH Memory Update Utility. 
 
You must record your CMOS SETUP parameters before updating the BIOS and set 
the CMOS parameters to default values after the update is complete, then 
re-enter the original values.  Erratic operation may result if the SETUP 
parameters are not set to default values.  You can set the CMOS parameters 
to default values by entering SETUP, going to the EXIT submenu and highlight
the 'Load Setup Defaults' option.  The CMOS memory map may change from BIOS
version to BIOS version, setting the parameters to default values will guarantee
the CMOS memory is updated correctly. 
 
See the file BIOINSTR.TXT for complete instructions on updating the BIOS. 
 
SHOWHDR.EXE:  This tool is provided to display header information
on the specified FLASH data image while running under Windows. 
 
Usage: SHOWHDR.EXE FLASH_data_image_filename 
 
IFLASH /P : DOS command line FLASH update utility 
IFLASH /X : Examine header information on the specified FLASH data image. 