Fertiges Bootimage mit intergriertem Flashtool + ASRock AMC_ConRoe865PE_div_5_4_1.6 Bios by ASRock_User für pc-treiber.net, powered by geekster.


Eine ausführlich Anleitung findet ihr hier:
http://www.pc-treiber.net/datenbank_artikel_24_HowTo-Bios-richtig-mit-Bootimages-flashen.html

Probleme bitte bei pc-treiber.net im Forum melden. Danke. 

Das Flashen geschieht auf eigene Gefahr.  

++
Das Bios stammt von AMC! 
++


Based on Version 1.6 of the original Bios.


====================================================================
AMC BIOS 1.1  5:4 				 Released 30.12.2006
====================================================================

Based on Version 1.6 of the original Bios.

====================================================================
Features:
====================================================================

Enables the 5:4 FSB/RAM Divider for ASRock ConRoe865PE motherboards.

====================================================================
How to:
====================================================================

1) Simply extract the AMC_ConRoe865_5_4.rom from the .zip file to a 
   folder on your harddrive. 

2) Download the AFU (AMI Flash Utility) from 
   http://www.pc-treiber.net/datei_download_76.html

3) Start the program and open the AMC_ConRoe865_5_4.rom from your  
   harddrive.

4) Make sure that 'program all blocks' is checked in the Setup of
   the AFU Utility. 

5) Press 'Flash' and reboot your computer.

====================================================================
IMPORTANT NOTICE - READ CAREFULLY BEFORE FLASHING
====================================================================

The setting for 5:4 divider WON'T SHOW UP IN THE BIOS MENU. You have
to check in windows whether it is working or not!! Try CPU-Z, Sandra
or Everest, for example. 

!!!!KEEP IN MIND, THAT YOUR PC IS STARTING WITH A DEFAULT OF 212 MHZ
RAM-CLOCK, RESULTING IN DDR 424!!!!

Also notice, that you *HAVE* to leave the RAM-Timings at:

[AUTO]-x-y-z! You can change everything except the CAS Latency! If 
you do so, the BIOS will probably override the 5:4 divider back to
3:2, but this ist *NOT* GUARANTEED! If you have bad RAM, don't know,
if your RAM can handle these speeds, then STAY AWAY FROM THIS BIOS!

You *CAN* change CAS Latency under windows, if you want to do:

Try i865Tweak : http://www.cpuid.org/download/Tw865.zip 
or  Memset : http://rv.page.cegetel.net.perso.cegetel.net/MemSet.zip

Keep in mind, that the BIOS settings are HARDCODED, if you are un-
satisfied with a 5:4 divider, you have to change and flash another 
BIOS, like the original one, or my 1:1 divider BIOS also available 
at http://www.pc-treiber.net/download_kategorie_26.html

====================================================================
DISCLAIMER 
====================================================================

- This mod-BIOS is a private project! 
- If you want to use it, use it at your *OWN* risk! 
- I am *NOT* responsible for any damage did to your hardware by the
  use of this BIOS, nor is AMI or ASRock!

  With flashing AMC_ConRoe865_5_4.rom to your BIOS, you agree to 
  these terms of use!

- AMC - Germany - November 2006

====================================================================
The TEAM (The good, the bad, the ugly ;-))
====================================================================

AMC     : Modder
pajaa   : Tester
BadFred : Tester
