:=========================================================================
: File name : nk12x.114
: File size : 1069186
: Version: 1.14
: Check Sum : 0B8C ECFA
: VGA OPROM Version:yj19938a_6.cfg
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 03/31/2008
: M/B Revision: DMT(Rev.C)
: Note : Base on NK12X.113 
:=========================================================================
1.Update AMD AGESA code to 3.1.8.0          
:=========================================================================
: File name : nk12x.113
: File size : 1069186
: Version: 1.13
: Check Sum : 0B8C F605
: VGA OPROM Version:yj19938a_6.cfg
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 03/26/2008
: M/B Revision: DMT(Rev.C)
: Note : Base on NK12X.112 
:=========================================================================
1.Fixed Crisis function can not work issue
:=========================================================================
: File name : nk12x.112
: File size : 1069186
: Version: 1.12
: Check Sum : 0B8D 7AC5
: VGA OPROM Version:yj19938a_6.cfg
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 02/21/2008
: M/B Revision: DMT(Rev.C)
: Note : Base on NK12X.111 
:=========================================================================
1. Update AMD AGESA code to 3.1.7.0
:=========================================================================
: File name : nk12x.111
: File size : 1069186
: Version: 1.10
: Check Sum : 0B8F A350
: VGA OPROM Version:yj19938a_6.cfg
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 02/15/2008
: M/B Revision: DMT(Rev.C)
: Note : Base on NK12X.110 
:=========================================================================
1.Add item for skip/halt System Event Log Full error during POST
:=========================================================================
: File name : nk12x.110
: File size : 1069186
: Version: 1.09
: Check Sum : 0B8F 5921
: VGA OPROM Version:yj19938a_6.cfg
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 01/30/2008
: M/B Revision: DMT(Rev.C)
: Note : Base on NK12X.109 
:=========================================================================
1.Fixed BIOS test suite 4.4.2 fail
2.Skip StrongRom Test               
3.Correct some string error 
:=========================================================================
: File name : nk12x.109
: File size : 1069186
: Version: 1.09
: Check Sum : 0B8D 04F6
: VGA OPROM Version:yj19938a_6.cfg
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 01/03/2008
: M/B Revision: DMT(Rev.C)
: Note : Base on NK12X.108 and update codebase to 1.36
:=========================================================================
1.Update Phoenix codebase to 1.36 
2.Update AMD AGESA code to 3.1.5.0
3.Modify AMD Errata 298 item to TLB Enable/Disable item
4.Correct MMIO overlap
:=========================================================================
: File name : nk12x.108
: File size : 1069186
: Version: 1.08
: Check Sum : 0B7B A136
: VGA OPROM Version:yj19938a_6.cfg
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 12/27/2007
: M/B Revision: DMT(Rev.C)
: Note : Base on NK12X.107 
:=========================================================================
1.Add Enable/Disable AMD Errata298 BIOS ITEM
:=========================================================================
: File name : nk12x.107
: File size : 1069186
: Version: 1.07
: Check Sum : 0B7D 46BB
: VGA OPROM Version:yj19938a_6.cfg
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 12/06/2007
: M/B Revision: DMT(Rev.C)
: Note : Base on NK12X.106 
:=========================================================================
1.Fixed ECC item garbage display 
2.Update AMD Agesa code to 3.1.4.0
3.Add Fan Sensor Configuration Function(Let User Select which fan need to monitor)         
4.Add Time zone setting for BMC
5.Hiding Virtual for ScorpioII
6.Correct SEL TimeStamp Error
7.Remove POST WatchDog item
8.correct display L2 cache size
9.Correct Set data as SW team Request
10.Fix BTS 4.2.1 error
11.Change string "GMT TIME Zone" to "BMC TimeZone"
:=========================================================================
: File name : nk12x.106
: File size : 1069186
: Version: 1.05
: Check Sum : 0B84 61CD
: VGA OPROM Version:yj19938a_6.cfg
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 11/09/2007
: M/B Revision: DMT(Rev.C)
: Note : Base on NK12X.105 
:=========================================================================
1.Correct DHCP function for ScorpioII
  feature\ipmi\common.600\cfglan.asm                     
:=========================================================================
: File name : nk12x.105
: File size : 1069186
: Version: 1.05
: Check Sum : 0B84 71D0
: VGA OPROM Version:yj19938a_6.cfg
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 10/04/2007
: M/B Revision: DMT(Rev.C)
: Note : Base on NK12X.104 and integrate with Phoenix codebase 1.21
:=========================================================================
1.Modify Spread Spectrum function
2.Remove Led Light off code in INT 19	    
3.Add PowerNow Enable / Disable item
4.Fixed some board will hange as initial HT Bus and show FF when Battery fail
5.Modify the summary screen feature
6.Modidfy ECC ITEMS
7.Remove OPROM_PLACEMENT parameter              
8.Remove "Err/Progress" item in sensor menu
:=========================================================================
: File name : nk12x.104
: File size : 1069058
: Version: 1.04
: Check Sum : 0B8A 27AD
: VGA OPROM Version:yj19938a_6.cfg
: PXE OPROM: 249.0542
: SATA OPROM:
: NVMM:4.073.19
: Release Date: 09/19/2007
: M/B Revision: DMT(Rev.C)
: Note : Base on NK12X.103
:==========================================================================
1.Remove set Lan speed code to avoid Scorpio II function invalid
2.1.Update AMD AGESA Code to 3.1.1.1 and Fixed AMD CPU(Rev.F) command buffer overlow
3.Set MSR Interrupt Pending and CMP-Halt Register (Offset C0010055)value as 0 (From AMD information)
4.Enable AMD Errata 281
5.Hide some bios setup item temporarily(advanced->chipset feature ->ECC due to Phoenix code bug)
:=========================================================================
: BIOS Revision: V1.03
: BIOS Checksum: 0B89 8817
: VGA OPROM Version: yj19938a_6.cfg
: PXE ROM:249.0542
: NVMM:4.073.19
: SATA OPROM:
: Release Date: 
: M/B Revision: DMT(Rev.C)
: Note:Based on nk12x.102
:==========================================================================
1.Update AMD AGESA Code to 3.1.10
2.Fixed BIOS item "After Power Failure set stay off" will cause console
  redirection function invalid
3.Fixed BIOS item "WakeOn Lan" set disable function invalid when 
  shutdown from Windows OS
4.Update PXE OPROM to 249.0542 to fix PXE function
  invalid on Giga mode
5.Update DXE Driver to fix WinPhlash64 can not flash issue
6.Remove Fru write command 
7.Update some files to fix OPMA mount two usb device issue
8.Remove AMD Errata 281 and update Nvidia NVMM to 4.073.19
9.Fixed some Bios Test Suite Error (Verson 3.5.6)
10.Disable AMD Errata 281
11.Update Some USB code to fixed install Linux will hang when OPMA Card On board by using usb-cdrom 
:=========================================================================
: BIOS Revision: V1.02
: BIOS Checksum: 0B9C CC37
: VGA OPROM Version: yj19938a_6.cfg
: Release Date: 08/06/2007
: M/B Revision: DMT(Rev.C)
: Note:Based on nk12x.101
:==========================================================================
1.Remove"WARNING: Non-Matching Processors - CPUs UP/DP/MP Capability Mismatch"
2.Change PXE ROM back to the same as bios 1.00 to fix pxe only work fine 
  when two nic plugged in	 
:=========================================================================
: BIOS Revision: V1.01
: BIOS Checksum: 0B9C 5876
: VGA OPROM Version: yj19938a_6.cfg
: Release Date: 07/09/2007
: M/B Revision: DMT(Rev.C)
: Note:Based on nk12x.100
:==========================================================================
1.Change VGA option rom to fix OPMA remote install Red Hat as4 up3 will has garbege display
2.Change PXE Rom
3.Support auto fan control
4.Change BIOS Version to 1.01         
5.Update AMD AGESA Code to 3.0.9.5          
6.Correct asl code to fix blue screen when install windows
7.Fixed AMD CPU(Rev.F) command buffer count over flow
8.Fix BIOS test suite error	     
9.Change Boot Sequence
10.ADD Memory ECC Item in bios setup          
:=========================================================================
: BIOS Revision: V1.00
: BIOS Checksum: 0B9E E562 
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.C)
: Note:Phoenix code base mcp55_2k8_rev1_dr_1_7.ZIP and integrate 12X080
:      From this bios nk12X can support AMD Dual Core and Quad Core
:      CPU at the same time.Comment start with OEMB001 
:==========================================================================
1.For Bring up           
2.Remove Phoenix 16 IDE Hard Drives Feature          
3.Include VGA OPROM        
4.Change GUI Module move from 080 BIOS rename old as GUI.bak         
5.Add Support 49LF080A Flash Part 
6.Fixed COM B Function cannot work
7.Modify PCI Routing for VGA Device
8.Remove S3 support and remove some unsed asl/asi code
9.Change the PCI-E Configuration to Match HW Design(16_1_1_1_1_8)
10.Enable LOGO
11.Add Server Page in Setup
12.Modify POST Screen
13.Add Spread Spectrum item in setup
14.Add IOMMU and Dram Bank Interleave in setup
15.Add support ADM1026 (move from nk12x.080)
16.Add PXE Retry function
17.Change CPU Number start from 1
18.Correct PCI-E 8X Routing
19.Put MAC Address in ADM1026 EEPROM
20.Add Wake On Lan Function
21.Display cpu and memory speed in post screen 
22.Remove the string"FOR EVALUATION ONLY. NOT FOR RESALE."
23.Change DMI information to 1.00 and fix DMI cannot change 
24. Add Workaround to Fix when plug PCI-Card and enter their utility the            "ESC" will not work
25.Add RTC WakeUp Function(Power Button)
26.Fix clear cmos system time and date will be cleared
27.Add workaround to fix some board will hang 29h when battery fail
28.Fixed HCT test "Unreported Memory and IO" will crash and fail        
29.Fixed HCT Test 'Enable/Disable Device IO" Error
30.Remove FDC Configuration
31.Remove LPT Configuration
32.Remove C State Configuration item
33.Add Detect OPMA Card Function , if OPMA Card is plugged in , hide
  HardwareMonitor item in bios , otherwis hide ipmi item in bios
34.Fixed RTC WakeUp Fuction invalide under Windows
35.Remov COM B IR Fucntion Selection
36.Support Server Management (Move from nk12x 080)          
37.Change AC Recovery Default Value as Enable
38.Fixed WOL Function invalid when connect to 1G switch
39.Correct WDT Function error
40.Fixed Disable USB , it will also disable second MAC
41.Add workaround to fix sometimes will hang as post 98h when OPMA plug in
42.Porting Lan Led Light
43.Disable GPIO/SMI at post code 08h
44.Remove PCIE Recovery Routine, due to nk12X don't need this
45.Remove the BMC/OPMA Device Revision in Setup and POST
46.Add Program BMC IP , Subnet Mask, GateWay BIOS, DHCP/Static  in 
  bios Setup Item
47.Fixed BIOS Check Error(4.4.0)            
48.Correct DR CPU MEM CLK Display Error 
49.Change After Power Failure as "Power on" "Last State" "Stay Off"
Change BIOS Version to V1.00         		
:=========================================================================
: BIOS Revision: V0.80
: BIOS Checksum:  
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.C)
: Note : Base on Code Base V0.54F1 
:==========================================================================
1.Add Support SST 49LF080A Flash Part
2.Change BIOS Version to 0.80 
:=========================================================================
: BIOS Revision: V0.54F1
: BIOS Checksum:  
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.C)
: Note : Base on Code Base V0.54E 
:==========================================================================
1.Add BMC IP Source information in BIOS setup       		 	         
2.Change BIOS Version to 054F1 
:=========================================================================
: BIOS Revision: V0.54E
: BIOS Checksum:  
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.C)
: Note : Base on Code Base V0.54B  and integrate it to Phoenix codebase 1.25
:==========================================================================
1.Correct BMC Lan Configuration Feature	         
2.Change BIOS Version to 054E 
:=========================================================================
: BIOS Revision: V0.54D
: BIOS Checksum:  
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.C)
: Note : Base on Code Base V0.54B  and integrate it to Phoenix codebase 1.25
:==========================================================================
1.Add Program BMC IP , Subnet Mask, GateWay BIOS, DHCP/Static  in 
  bios Setup Item       
2.Change BIOS Version to 054C 
:=========================================================================
: BIOS Revision: V0.54C
: BIOS Checksum:  
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.C)
: Note : Base on Code Base V0.54B  and integrate it to Phoenix codebase 1.25
:==========================================================================
1.Correct some coding error 
2.Change BIOS Version to 054C 
:=========================================================================
: BIOS Revision: V0.54B
: BIOS Checksum:  
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.C)
: Note : Base on Code Base V0.54A  
:==========================================================================
1.Remove the BMC/OPMA Device Revision in Setup and POST 
2.Remove Total Cache Size and recovery back to show L2 Cache Size Per CPU
3.Implement AMD Errata#157 SVM Patch
4.Fixed BIOS CHECK ERROR (4.3.1)       
5.Change BIOS Version to 054B 
:=========================================================================
: BIOS Revision: V0.54A
: BIOS Checksum:  
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.C)
: Note : Base on Code Base V0.54 
:==========================================================================
1.Fixed MMIO Overlap found by AMD QT (BIOS CHECK 4.3.1)
2.Fixed BIOS CHECK ERROR found by AMD QT (BIOS CHECK 4.3.1)
3.Fixed Post incorrect CPU Cache Size
4.Change BIOS Version to V0.54A
:=========================================================================
: BIOS Revision: V0.54
: BIOS Checksum:  
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.C)
: Note : Base on Code Base V0.53  and integrate it to Phoenix codebase 1.25
:==========================================================================
1.Remove PCIE Recovery Routine, due to nk12X don't need this
2.Fixed BIOS Check Error (BIOS check verson 4.0.3, Agesa code 2.08.00)
3.Remove Fru Command
4.Remove unused code for nk12x
5.Update Phoenix USB 2.0 Split Transction Code (Integrate with Phoenix codebase1.25) also remove OEM58 workaround for KVM Issue
Change BIOS Version to 0.54             
:=========================================================================
: BIOS Revision: V0.53
: BIOS Checksum:  
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.C)
: Note : Base on Code Base V0.52C1 (Phoenix Code Base----B_977001_1.1)
:==========================================================================
1.Disable GPIO/SMI at post code 08h
2.Fixed GPIO/SMI Pin initial error
3.Correct some 1026 initial value
4.Change Enable SMI/GPIO Point 
5.Remove Lan Led Porting to post code 49 (PCIINIT)       
6.Correct some codeing error 
7.Fixed Sometimes lan will fail for Scorpio II  	
:=========================================================================
: BIOS Revision: V0.52C1
: BIOS Checksum:  
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.C)
: Note : Base on Code Base V0.52C (Phoenix Code Base----B_977001_1.1)
:==========================================================================
1.Correct some 1026 initial value when OPMA not onBoard
2.Change PowerOnAndReset Command Point
3.Change to only check cpu1 status when system fault assertion         		
Change BIOS Version to V0.52C1  		   	
:=========================================================================
: BIOS Revision: V0.52C
: BIOS Checksum:  
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.C)
: Note : Base on Code Base V0.52B (Phoenix Code Base----B_977001_1.1)
:==========================================================================
1.Chang SMI/GPIO for Rev.C 		  
Change BIOS Version to V0.52B  		   	
:=========================================================================
: BIOS Revision: V0.52B
: BIOS Checksum:  
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.B)
: Note : Base on Code Base V0.52A (Phoenix Code Base----B_977001_1.1)
:==========================================================================
1.Modify BIOS Setup Screen
2.Modify Post Screen
3.Fixed Disable USB , it will also disable Second MAC (MAC1)
4.Add workaround to fix sometimes will hang as post 98h when OPMA plug in	  
Change BIOS Version to V0.52B  
:=========================================================================
: BIOS Revision: V0.52A
: BIOS Checksum:  
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.B)
: Note : Base on Code Base V0.52 (Phoenix Code Base----B_977001_1.1)
:==========================================================================
1.Fixed Get Mac From OPMA Error	  
Change BIOS Version to V0.52A  		   	
:=========================================================================
: BIOS Revision: V0.52
: BIOS Checksum: 0435 D337 
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.B)
: Note : Base on Code Base V0.51B (Phoenix Code Base----B_977001_1.1)
:==========================================================================
1.Correct SetSystemTypeID Error
2.ServerMangement support (OPMA OnBoard)	  
3.Add fake smi, this is test for servermanagement
4.Correct WDT Function Error (Reboot Issue)
5.Fixed AMD BIOS Check Error (BIOS Check Verion is 4.0.3)          
6.Fixed random hang at POST code 0x55h during warm boot while USB legacy function support enable.
7.Change BIOS Version to V0.52  		   	
:=========================================================================
: BIOS Revision: V0.51B
: BIOS Checksum:  
: VGA OPROM Version: yj19938a.005
: Release Date: 
: M/B Revision: DMT(Rev.B)
: Note : Base on Code Base V0.51 (Phoenix Code Base----B_977001_1.1)
:==========================================================================
1.Fixed RTC WakeUp Function invalide under Windows
2.Remove COM B IR Fucntion Selection
3.Add workaround to fix Some boards will hang at post code 29 when Battery fail
4.Support ServerManagement (without OPMA on board)
5.Change VGA Option Rom 
6.Change AC Recovery Default Value to Enable
7.Correct VCore string in hardware monitor menu 
8.Change GUI Level From 2 to 1 and fixed password function invalid in bios setup
9.Correct HardWare Monitor Item Value display error
10.Implement HardWare Monitor Formula
11.Change DMI "System Information" Product Name as "NK12X"
12.Fixed WOL function invalid when connect to 1G switch
13.Change BIOS Version to V0.51B	
:=========================================================================
: BIOS Revision: V0.51
: BIOS Checksum: 04E5 382E 
: VGA OPROM Version: yj616d1.tst(with DVI support)
: Release Date: 
: M/B Revision: DMT(Rev.B)
: Note : Base on Code Base V0.50 (Phoenix Code Base----B_977001_1.1)
:==========================================================================
1.Correct Lan 2 Led Light 
2.Recovery the Mouse asl code
3.Change the VGA OPROM to yj616d1.tst(get from NM46X)
4.Add Detect OPMA Card Function , if OPMA Card is plugged in , hide
  HardwareMonitor item in bios , otherwis hide ipmi item in bios
5.Correct DDIO Value in HWMON ITEM
6.Remove program username, password, IPAddress, and MAC Address to BMC 
7.Remove LPT Port item
:=========================================================================
: BIOS Revision: V0.50B
: BIOS Checksum: 0413 E326  
: VGA OPROM Version: yj616d.tst(with DVI support)
: Release Date: 
: M/B Revision: DMT(Rev.B)
: Note : Base on Code Base V0.50 (Phoenix Code Base----B_977001_1.1)
:==========================================================================
1.Correct Lan 2 Led Light 
:=========================================================================
: BIOS Revision: V0.50
: BIOS Checksum: 0414 13F6
: VGA OPROM Version: yj616d.tst(with DVI support)
: Release Date: 
: M/B Revision: DMT(Rev.B)
: Note : Base on Code Base V0.06
:==========================================================================
1.Change PHY 1 Physical Address to 00010h
2.Remove floppy configuration (due to Rev.B doesn't have floppy)
3.Remove LPT Port Configuration(due to NK12X doesn't LPT Port)
4.Remove C State Configuration item and add "After Power Failure" item
:=========================================================================
: BIOS Revision: V0.06
: BIOS Checksum: 0414 1F00 
: VGA OPROM Version: yj616d.tst(with DVI support)
: Release Date: 10/11/2006
: M/B Revision: DVT(Rev.A)
: Note : Base on Code Base V0.05D (Phoenix Code Base----B_977001_1.1)
:==========================================================================
1.Add RTC WakeUp Function(Power Button)
2.Fix clear cmos system time and date will be cleared
3.Remove PassWord on Boot item
4.Fixed HCT test "Unreported Memory and IO" will crash and fail
5.Workaround HCT test "PCI Compliance" fail,also add one MCFG enable/disable              item and need to select enable when hct test under Windows, but when to use             linux OS , need to select disable
6.Fixed HCT test "Enable/Disable Device IO"
7.Change the GUI Level From 1 to 2 temporary, rename GUI levl1 folder as GUI1
:=========================================================================
: BIOS Revision: V0.05D
: BIOS Checksum: 0438 4195 
: VGA OPROM Version: yj616d.tst(with DVI support)
: Release Date: 09/21/2006
: M/B Revision: DVT
: Note : Base on Code Base V0.05C (Phoenix Code Base----B_977001_1.1)
:=======================================================================
1.Change Lan Port Led Light to Match NEW POR Spec(0.99)
2. Change GUI Level from 2 to 1 , due to want set/make password
   in bios setup security function work correct, change a new gui
   folder and rename old as gui.bak
3.Add Workaround to Fix when plug PCI-Card and enter their utility the "ESC" will not work
:======================================================================
: BIOS Revision: V0.05C
: BIOS Checksum: 0417 AD95 
: VGA OPROM Version: yj616d.tst(with DVI support)
: Release Date: 09/19/2006
: M/B Revision: DVT
: Note : Base on Code Base V0.05 (Phoenix Code Base----B_977001_1.1)
:=======================================================================
1.Fixed DMI String cannot Change Issue
2.Change Lan Port Led Light to Match POR Spec
3.Hidden SATA2 and SATA3 in setup due to nk12x don't have these
4.Change the PCI-E Configuration to Match HW Design(16_1_1_1_1_8) because
  mcp55v pro just only this configuration...this is different from mcp55v
  and fixed some PCI-E Card cannot Detect
:======================================================================
: BIOS Revision: V0.05
: BIOS Checksum: 0417 5395 
: VGA OPROM Version: yj616d.tst(with DVI support)
: Release Date: 09/04/2006
: M/B Revision: DVT
: Note : Base on Code Base V0.04A (Phoenix Code Base----B_977001_1.1)
:=======================================================================
1.Add Wake On Lan Function
2.Modify CPU Package to L1 in bootblok tip      	
3.Display cpu and memory speed in post screen 
4.Modify FDA TYPE to match BIOS SPEC
5.Fixed BIOSCHECK Error	
6.Fixed USB1.1 work not correctly 	
7.Remove the string"FOR EVALUATION ONLY. NOT FOR RESALE." on post
:=====================================================================
: BIOS Revision: V0.04A
: BIOS Checksum: 0416  4142
: VGA OPROM Version: yj616d.tst(with DVI support)
: Release Date: 08/23/2006
: M/B Revision: DVT
: Note : Base on Code Base V0.04 (Phoenix Code Base----B_977001_1.1)
:=======================================================================
1.Correct PCI-E 8x slot Routing 
2.Change BIOS Version to V0.04A
:======================================================================
: BIOS Revision: V0.04
: BIOS Checksum: 0416 1E61
: VGA OPROM Version: yj616d.tst(with DVI support)
: Release Date: 08/23/2006
: M/B Revision: DVT
: Note : Base on Code Base V0.03 (Phoenix Code Base----B_977001_1.1)
:=======================================================================
1.Enable startup screen with Arima logo
2.Correct VGA Routing 
3.Change BIOS Version to V0.04
:======================================================================

: BIOS Revision: V0.03
: BIOS Checksum: 03F8 DA7A 
: VGA OPROM Version: yj616d.tst(with DVI support)
: Release Date: 08/21/2006
: M/B Revision: DVT
: Note : Base on Code Base V0.02 (Phoenix Code Base----B_977001_1.1)
:=======================================================================
1.Modify BIOS Setup Screen
2.Set Interrupt Mode Default to APIC Mode	
3.Set Legacy USB Support default to Enable	
4.Add Server page in Setup
5.Add NOKBERR ITEM in Setup
6.Add Spread Spectrum item in Setup	
7.Fixed Enable Spread Spectrum will hang 98h	
8.Add IOMMU and Dram Bnak Interleave(default to auto) in setup	
9.ADD ADM1026 function in setup
10.Put MAC address in ADM1026 EEPROM and add PXE retry function
11.Change Raid OPROM to nvraid.sg to avoid show SGPIO init fail
12.Change VGA OPROM as yj616d.tst(with DVI support)
13.Change CPU Number start from 1 
14.Change BIOS Version to NK12X V003	
:======================================================================
: BIOS Revision: V0.02
: BIOS Checksum: 03F8 8B05 
: VGA OPROM Version: yj616d.200(yj616d.002)
: Release Date: 08/17/2006
: M/B Revision: DVT
: Note : Base on Code Base V0.01 (Phoenix Code Base----B_977001_1.1)
:===========================================================
1.Fixed hang when install linux 	
:===========================================================
: BIOS Revision: V0.01 (For bring up)
: BIOS Checksum: 03F7 F0D6 
: VGA OPROM Version: yj616d.200(yj616d.002)
: Release Date: 08/06/2006
: M/B Revision: DVT
: Note : Base on Phoenix Code Base----B_977001_1.1  
:===========================================================
0. Modify the DIMM Address for NK12X Project	 
1. Modify the CPU Package type to Server Platform         	  
2. Modify the HT link for NK12X Project	 
3. Support 49LF040B Flash Part	
4. Modify PCI Routing for VGA Device
5. Change VGA Option Rom to yj616d.200(yj616d.002) VGA memory frequency 200MHz
6. Change AMD HT MMIO to Link 1 , or it will hange at post 45h	 
7. Remove S3 support and remove some unsed asl/asi code	          
8. Fixed COM B Function cannot work
         