:=========================================================================
: File name : nk14x.102
: File size : 1069170
: Version: 1.02
: Check Sum : 0B90 44CD
: VGA OPROM Version:yj24122a.003
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 03/31/2008
: M/B Revision: Rev.B
: Note : Base on NK14X V1.01
:==========================================================================
1.Update AMD AGESA code to 3.1.8.0
:=========================================================================
: File name : nk14x.101
: File size : 1069170
: Version: 1.01
: Check Sum : 0B90 61D2
: VGA OPROM Version:yj24122a.003
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 03/26/2008
: M/B Revision: Rev.B
: Note : Base on NK14X V1.00
:==========================================================================
1.Fixed Crisis function can not work issue
:=========================================================================
: File name : nk14x.100
: File size : 1069170
: Version: 1.00
: Check Sum : 0B90 72D3
: VGA OPROM Version:yj24122a.003
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 03/12/2008
: M/B Revision: Rev.B
: Note : Base on NK14X V0.54
:==========================================================================
Base on 0.54 and change BIOS to 1.00 for FAI stage
:=========================================================================
: File name : nk14x.054
: File size : 1069170
: Version: 0.54
: Check Sum : 0B90 6ED4
: VGA OPROM Version:yj24122a.003
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 02/21/2008
: M/B Revision: Rev.B
: Note : Base on NK14X V0.53
:==========================================================================
1.Update AMD Agesa code to 3.1.7.0
:=========================================================================
: File name : nk14x.053
: File size : 1069170
: Version: 0.52
: Check Sum : 0B91 6B6A
: VGA OPROM Version:yj24122a.003
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 01/30/2008
: M/B Revision: Rev.B
: Note : Base on NK14X V0.52
:==========================================================================
1.Skip StrongRom Test
2.Correct some string error 
:=========================================================================
: File name : nk14x.052
: File size : 1069170
: Version: 0.52
: Check Sum : 0B8F 6542
: VGA OPROM Version:yj24122a.003
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 01/04/2008
: M/B Revision: Rev.B
: Note : Base on NK14X V0.51 and update Phoenix codebase to 1.36
:==========================================================================
A.Update Phoenix codebase to 1.36
1.Correct MMIO Overlap
2.Add TLB Enable/Disable item
3.Update Agesa code to 3.1.5.0            
:=========================================================================
: File name : nk14x.051
: File size : 1069170
: Version: 0.51
: Check Sum : 0B80 2211
: VGA OPROM Version:yj24122a.003
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 12/06/2007
: M/B Revision: Rev.B
: Note : Base on NK14X V0.50
:==========================================================================
1.correct display L2 cache size(Per AMD's request) 
2.correct CPU 2356 BTS error(for AMD's validataion)
3.Correct SEL data as SW/IPMI team Request
4.Update AMD AGESA code to 3.1.4.0
5.Fixed CPU 2350 BTS error, BTS's version is 4.2.1
:=========================================================================
: File name : nk14x.050
: File size : 1069170
: Version: 0.10
: Check Sum : 0B84 5C20
: VGA OPROM Version:yj24122a.003
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 11/21/2007
: M/B Revision: Rev.B
: Note : Base on NK14X V0.10
:==========================================================================
1.Update AMD Agesa code to 3.1.3.1
2.Add Fan Sensor Configuration Function(Let User Select which fan need to monitor)
3.Correct DHCP function for ScorpioII
4.Add Time Zone Setting for BMC
5.Hiding Virtual for ScorpioII
6.Correct SEL TimeStamp Error
7.Remove POST WatchDog item
Change BIOS to 0.50
:=========================================================================
: File name : nk14x.010
: File size : 1069170
: Version: 0.10
: Check Sum : 0B88 7ED8
: VGA OPROM Version:yj24122a.003
: PXE OPROM: 249.0542
: SATA OPROM:9.71
: NVMM:4.073.19
: Release Date: 10/03/2007
: M/B Revision: Rev.B
: Note : Base on NK14X  V0.09 and integrate wiht Phoenix codebase 1.21
:==========================================================================
1.Remove "Err/Progress" item in sensor menu
2.Modify the summary screen feature
3.Modidfy ECC ITEMS
4.Change compiler tool to MASM 8.0
:=========================================================================
: File name : nk14x.009
: File size : 1069058
: Version: 0.09
: Check Sum : 0B90 4A04
: VGA OPROM Version:yj24122a.003
: PXE OPROM: 249.0542
: SATA OPROM:
: NVMM:4.073.19
: Release Date: 09/19/2007
: M/B Revision: Rev.B
: Note : Base on NK14X  V0.08
:==========================================================================
1. Add PowerNow Enable / Disable item
2.Disable FW Ready GPIO PIN temporary             
3.Fixed some boards will hang post code 29	  
4.Fixed some board will hange as initial HT Bus and show FF when Battery fail	   
5.Enable FW Ready GPIO PIN
6.Fixed FW Ready SMI invalid
7.Correct System Type error when FW Ready
8.Correct Enhanced SATA signal
9.Set MSR Interrupt Pending and CMP-Halt Register Offset C0010055 value as 0 (From AMD information)
10.Enable AMD Errata 281
11.Fixed Rev.F CPU BTS Error
12.Hide some bios setup item temparily(due to Phoenix code bug)             
===============================================================================================
: BIOS Revision: V0.08
: BIOS Checksum:  0B8D F2D3
: VGA OPROM Version:yj24122a.003
: PXE OPROM: 249.0542
: SATA OPROM:
: NVMM:4.073.19
: Release Date: 09/04/2007
: M/B Revision: Rev.B
: Note : Base on NK14X  V0.07
:==========================================================================
1.Remove Led Light off code in INT 19
2.Modify Spread Spectrum function
3.Fixed System hang when set sata controller as "Disabled"
4.Update AMD AGESA Code to 3.1.1.1 and Fixed AMD CPU(Rev.F) command buffer count over flow            
5.Correct Fan Enable function for Rev.B(HW Design Change)
:=========================================================================
: BIOS Revision: V0.07
: BIOS Checksum:  0B8E 80CA
: VGA OPROM Version:yj24122a.003
  PXE OPROM: 249.0542
  SATA OPROM:
: Release Date: 08/24/2007
: M/B Revision: DVT(Rev.A && Rev.B)
: Note : Base on NK14X  V0.06
:==========================================================================
1.Remove AMD Errata 281 and update Nvidia NVMM to 4.073.19
2.Disable AMD Errata 281
3.Update Some USB code to fixed install Linux will hang when
  OPMA Card On board

:=========================================================================
: BIOS Revision: V0.06
: BIOS Checksum:  0B91 EE52
: VGA OPROM Version:yj24122a.003
  PXE OPROM: 249.0542
  SATA OPROM:
: Release Date: 08/17/2007
: M/B Revision: DVT(Rev.A && Rev.B)
: Note : Base on NK14X  V0.05
:==========================================================================
1.Update some files to fix OPMA mount two usb device issue
2.Fix some AMD BIOS test suite3.5.6 fail for Barcelona Bx cpu
3.Update PXE OPROM to 249.0542 to fix PXE function
  invalid on Giga mode
4.Adjust SATA Register to enhance signal (add SATA1 and SATA2 detection)
5.Fixed Console Redirection function valid when After Power 
  failue item set as "stay off"
6.Update DXE Driver to fix WinPhlash64 can not 
  flash issue 
7.Remove Fru write command  
8.Remove setlan speed code 
:=========================================================================
: BIOS Revision: V0.05
: BIOS Checksum:  0B93 3AE3
: VGA OPROM Version: yj24122a.003
: Release Date: 08/10/2007
: M/B Revision: DVT(Rev.A)
: Note : Base on NK14X  V0.04
:==========================================================================
1.Update AMD Agesa code to 3.1.1.0 
2.Change New VGA Option rom to fix no DVO output            
3.Correct HW Monitor Fan item            
4.Fixed Performance test tool PassMark show warning message
5.Adjust SATA register to enhance the signal           
:=========================================================================
: BIOS Revision: V0.04
: BIOS Checksum:  0B9B 111D
: VGA OPROM Version: 
: Release Date: 07/30/2007
: M/B Revision: DVT(Rev.A)
: Note : Base on NK14X  V0.03
:==========================================================================
1.Hidden SATA2 and SATA3 item when disable SATA1 and modify help
  description
2.Fix 4Rank DIMM issue and Fix 2Rank DIMM speed down to 400 Mhz  
3.Fix Wake on lan disabled still can wake up when enter S5 from Windows
4.Correct the summary screen to match HW spec
:=========================================================================
: BIOS Revision: V0.03
: BIOS Checksum:  0BA2 7FE3
: VGA OPROM Version: 
: Release Date: 07/19/2007
: M/B Revision: DVT(Rev.A)
: Note : Base on NK14X  V0.02
:==========================================================================
1.Remove unsed device code  	  
2.Remove iommu item and unsed item in bios setup
3.Correct DMI information error
4.Change system id to match 14X
5.Remove -12V item in 1026 bios item
6.Fixed AMD CPU(Rev.F) command buffer count over flow
7.Fix BIOS test suite error
8.Remove"WARNING: Non-Matching Processors - CPUs UP/DP/MP Capability Mismatch"
9.Change bios version to 0.03  
:=========================================================================
: BIOS Revision: V0.02
: BIOS Checksum:  0B9D 151B
: VGA OPROM Version: yj19895a.001
: Release Date: 07/13/2007
: M/B Revision: DVT(Rev.A)
: Note : Base on NK14X  V0.01
:==========================================================================
1.Update AMD AGESA CODE to 3.0.9.5         
2.Correct asl code to fix blue screen when install windows           
3.Add ECC Item in bios setup            
4.Change bios version to 0.02            
5.Correct Legacy IO error            
6.Porgram Fan Enable Pin GP35 as gpio pin
7.Fix 4 Rank DIMM Sizing Error
8.Remove IDE item in bios setup                
::=========================================================================
: BIOS Revision: V0.01
: BIOS Checksum: 0BA8 D9c5
: VGA OPROM Version: yj19895a.001
: Release Date: 06/26/2007
: M/B Revision: DVT(Rev.A)
: Note : Base on NK12X V1.00
:==========================================================================
1.Change HT Routing
2.Change VGA Option Rom 
3.Change PXE Oprom  
4.Add Support 4 Rank DIMM
5.Display 3 SATA Controller in setup
6.Support Server Management for 14X 
7.Change BIOS DMI Version to V0.01
8.Support auto fan function and fan_enable at post code 86h          
:=========================================================================