ATI RC410/RC410L (RadeonXpress 200) chipset (Socket LGA775) - DDR II RAM 
microATX Motherboard

Award BIOS


A0413.BIN 	BIOS for (ATI RadeonXpress 200 RC410/L + ATI IXP450 + Winbond IO Chip)
		[with onboard VGA controller], Clock Gen ICS951413
		* with Hardware Monitor 
		* with STR (Suspend-To-RAM)
		* with onboard LAN
		* with 6 Channel AC97 Audio

A0413_A.BIN 	BIOS for (ATI RadeonXpress 200 RC410/L + ATI IXP450 + Winbond IO Chip)
		[with onboard VGA controller], Clock Gen ICS951413
		* with Hardware Monitor 
		* with STR (Suspend-To-RAM)
		* with onboard LAN
		* with 8 Channel HD Audio

A0413_B.BIN 	BIOS for (ATI RadeonXpress 200 RC410/L + ATI IXP450 + Winbond IO Chip)
		[with onboard VGA controller], Clock Gen ICS951413
		* with Hardware Monitor 
		* with STR (Suspend-To-RAM)
		* with onboard LAN
		* with 8 Channel HD Audio
		* No COM Port

.4MBit Flash
.Aug/2006 built core
.Initial Mass Production Release
(Aug/2006)

.4MBit Flash
.Sept/2006 built core
.Correct CPU temperature display figure error
.Improved DDR-2 667 RAM compatibility
(Sept/2006)

.4MBit Flash
.Oct/2006 built core
.Added PXE LAN BootROM function
(Oct/2006)

.4MBit Flash
.Feb/2007 built core
.Fixed Surroundview failure
.Fixed PS/2 Keyboard detection issue
.Fixed Window Vista Device Manager (!) mark issue
(Feb/2007)

.4MBit Flash
.April/2007 built core
.Removed PXE LAN BootROM function (due to size limitation)
.Updated for support of new CPUs
(April/2007)