Nvidia MCP73V/PV chipset (Socket 775), ATX / mATX

Award BIOS


N0714WZT.BIN	BIOS for MCP73V/PV, Winbond Super IO
		* With STR (Suspend-To-RAM)
		* With Hardware Monitor 
		* With LAN on board
		* With 8-Ch HD Audio
		* Zotac Full Screen Powerup Logo

.8Mbit Flash
.2007/Oct built core 
.Initial mass production release
(Oct/2007)

.8Mbit Flash
.2007/Nov built core 
.Fixed CPU Temperature issue
(Nov/2007)

.8Mbit Flash
.2007/Nov built core 
.Fixed power up display failure
.Fixed system temperature issue
(Nov/2007)

.8Mbit Flash
.2007/Dec built core 
.Fixed the CMOS Error after S3 Resume
(Dec/2007)

.8Mbit Flash
.2007/Dec built core 
.Changed CMOS Default Chipset Voltage to 1.35V
(Jan/2008)

.8Mbit Flash
.2008/July built core 
.Added IGPU overclocking function
(July/2008)