Nvidia MCP73V/PV chipset (Socket 775), Mini-ITX

Award BIOS


N1217_Zc.BIN	BIOS for MCP73V/PV, Winbond Super IO
		* for older PCB version, without STR (Suspend-To-RAM) hardware function
		* Zotac Full Screen Powerup Logo

N1217_Zb.BIN	BIOS for MCP73V/PV, Winbond Super IO
		* for newer PCB version-20 (str_back.jpg), with STR (Suspend-To-RAM) hardware function (str_front.jpg)
		* Zotac Full Screen Powerup Logo


.8Mbit Flash
.2008/July built core 
.Initial mass production release
(July/2008)

.8Mbit Flash
.2008/July update built
.Added IGPU overclocking function
(July/2008)

.8Mbit Flash
.2008/Oct update built
.Corrected detection on new stepping Q9550 CPU
(Oct/2008)

.8Mbit Flash
.2008/Dec update built
.Corrected LAN Card issue after power failure
.Added support for STR (Suspend-To-RAM) on newer PCB version-20 shipment
.Added memory voltage control option
.(Dec/2008)

.8Mbit Flash
.2009/Dec update built
.Added support on newer Flash (BIOS) IC types
.Added support for new CPUs
.Fixed CMOS Alarm Wake-Up [Day 0 = Everyday] selection failure issue
.(Dec/2009)



Remark :
======
The STR (Suspend-To-RAM) function is only applicable to newer PCB version-20 shipment.
