@SCREEN
{
|DESCRIPTION|HT VGA (800x600) 16-Color for Variable Frequency Monitors
|SHORT DESCR|HT VGA (800x600)
|FILENAME|SD800.VGA
|SRC DISK|HT VGA Driver Disk
|FONT DISK|GEM SCREEN DISK #2
|FNT WILDCRD|*.VGA
|LONG DESCRP|
Choose this entry if you are using a Variable Frequency
Monitor and the HT VGA card.  This display offers a
resolution of 800 horizontal by 600 vertical pixels.
}
{
|DESCRIPTION|HT VGA (1024x768) 16-Color for Variable Frequency Monitors
|SHORT DESCR|HT VGA (1024x768)
|FILENAME|SD1024C.VGA
|SRC DISK|HT VGA Driver Disk
|FONT DISK|GEM SCREEN DISK #2
|FNT WILDCRD|*.VGA
|LONG DESCRP|
Choose this entry if you are using a Variable Frequency
Monitor and the HT VGA card.  This display offers a
resolution of 1024 horizontal by 768 vertical pixels.
}

