
TABLE OF CONTENTS
-----------------

   I. Files on Disk
  II. Updates/Additional Information



I. FILES ON DISK
----------------

   Utilities
   ---------

SETUP	 EXE - Decompression utility to load software.
CLR	 COM - Clear screen utility for enhanced text modes.
ESU	 COM - Enhanced text mode selection utility.
README	 COM - Types file README.TXT.
README	 TXT - This file.
HTVGA	 EXE - Screen save and emulation utility.
ALTPARM  EXE - Alternate monitor parameter utility.
ALTPARM  DAT - Data file for ALTPARM.EXE
ERGO600  ALT - Parameter file: 800 x 600 at 72 Hz.
ERGO480  ALT - Parameter file: 640 x 480 at 72 Hz.
ERGO768  ALT - Parameter file: 1024 x 768 at 62.5 KHz/72 Hz.
ERGO768A ALT - Parameter file: 1024 x 768 at 58.1 KHz/72 Hz.
VESA1K70 ALT - Parameter file: 1024 x 768 at 70 Hz.
76HZ480  ALT - Parameter file: 640 x 480 at 76 Hz.
76HZ600  ALT - Parameter file: 800 x 600 at 76 Hz.
56HZ600  ALT - 800 x 600 for 56 Hz monitors such as NEC 2A.
NANA9070 ALT - Parameter file for Nanao 9070.
NEC4D	 ALT - Parameter file for NEC MultiSync 4D.
NEC4FG	 ALT - Parameter file for NEC MultiSync 4FG.
CM1440	 ALT - Parameter file for Seiko 1440.
MITS6605 ALT - Parameter file for Mitsubishi 6605.
SONY1304 ALT - Parameter file for Sony 1304.
NANA8060 ALT - Parameter file for Nanao 8060.
NANA9500 ALT - Parameter file for Nanao 9500.
HTVESA	 COM - VESA Bios Extension TSR.


   Lotus 2.0
   ---------

GD720V20 DRV - 720 x 540 graphics driver.
GD800V20 DRV - 800 x 600 graphics driver.
VD80X60  DRV - 80 x 60 text driver.
VD100X60 DRV - 100 x 60 text driver.
VD132X25 DRV - 132 x 25 text driver.
VD132X43 DRV - 132 x 43 text driver.


   Word Perfect 5.0
   ----------------

WP800	WPD - 800 x 600  - 16 color graphics driver.
WP1KC16 WPD - 1024 x 768 - 16 color graphics driver.


   Word Perfect 5.1
   ----------------

OEMGRAPH VRS - Graphics driver file.
OEMTEXT	 VRS - Text driver file.


   Word 5.x
   --------

VIDSETUP EXE - Resolution setup program.
SCREEN	 VID - Driver file.


   GEM/3 & Ventura
   ---------------

GEMSETUP TXT - GEM Driver Install data file.
SD800	 VGA - GEM & Ventura 800 x 600 graphics driver.
SD1024C  VGA - GEM & Ventura 1024 x 768 graphics driver.
VP2_0	 TXT - Ventura v2.0 driver Install data file.
VPINST_2 EXE - Ventura v2.0 driver Install program.


   AutoCAD
   -------

VGAREL11 COM - AutoCAD 9, 10 and 11 Real Mode driver.
R11INST  EXE - AutoCAD 11 installation program.
ADIDISP	 EXP - AutoCAD 386 Protected Mode driver.


   CADVANCE
   --------

GS1024	 DRV - 1024 x 768 16 color driver.
GS800	 DRV - 800 x 600 16 color driver.


   P-CAD
   -----

DPCAD1K	 DRV - 1024 X 768 with 16 colors.
DPCAD640 DRV - 640 x 480 with 16 colors.
DPCAD720 DRV - 720 x 540 with 16 colors.
DPCAD800 DRV - 800 x 600 with 16 colors.


   Generic CADD
   ------------

GCAD1024 VGD - 1024 x 768 with 16 colors.
GCAD2480 VGD - 640 x 480 with 256 colors.
GCAD2600 VGD - 800 x 600 with 256 colors.


   VersaCAD Design
   ---------------

VCAD1024 EXE - 1024 x 768 with 16 colors.
VCAD800	 EXE - 800 x 600 with 16 colors.
VCAD53	 CFG - VersaCAD 5.3 configuration file.
VCAD54	 CFG - VersaCAD 5.4 configuration file.


   VersaCAD/386
   ------------

VCAD1KP	 EXE - VersaCAD/386 1024 x 768 with 16 colors.
VCAD386	 CFG - VersaCAD/386 configuration file.


   Presentation Manager
   --------------------

MONMS	 DLL - Monitor file for NEC MultiSync monitors.
MON9070  DLL - Monitor file for Nanao 9070 monitors.
MONMS2A  DLL - Monitor file for NEC MultiSync 2A monitors.
MONXL	 DLL - Monitor file for NEC MultiSync XL monitors.
MONXLI   DLL - Monitor file for NEC XL (1024x768 interlaced mode) monitors.
MONMS2	 DLL - Monitor file for MultiSync II monitors.
MONPLUS  DLL - Monitor file for MultiSync Plus monitors.
MONPLUSI DLL - Monitor file for NEC Plus (1024x768 interlaced mode) monitors.
MON8060  DLL - Monitor file for Nanao 8060 monitors.
MON9070I DLL - Monitor file for NANAO 9070 (1024x768 interlaced mode).
MONSONY  DLL - Monitor file for Sony monitors.
MONSONYI DLL - Monitor file for SONY Multiscan (1024x768 interlaced mode).
MONXLO	 DLL - Monitor file for old MultiSync XL monitors.
VGA640	 DLL - 640 x 480 16 color driver file.
VGA720	 DLL - 720 x 540 16 color driver file.
VGA800	 DLL - 800 x 600 16 color driver file.
VGA1024  DLL - 1024 x 768 16 color driver file.



II. UPDATES/ADDITIONAL INFORMATION
------------------------------------

   Windows 3.1 Driver Installation
   -------------------------------

NOTE: This Windows installation procedure assumes that you have already
      used the SETUP utility to extract the Windows driver off utility
      disk and have installed them to the Window's SYSTEM directory.
      If you have not done so, please do so now before proceeding.

1) Install Windows using "VGA" as the display option.
   Choosing another driver will lead to incorrect results.

2) While running Windows in VGA mode, select the CONTROL PANEL icon
   in the MAIN program group.  Next select the HTDISPLAY icon. 

3) Select the desired color depth, supported font size, and supported
   screen resolution.  When the desired display configuration is
   set, select OK to set the configuration.

4) Next, you will be prompted to either use the CURRENT screen 
   drivers or NEW screen drivers from drive A.  Select the appropriate
   option.

5) Hit RESTART to run Windows in your new display configuration.

In the future, to change the display configuration repeat steps
2, 3, 4, and 5.


   IBM OS/2 2.X Driver Installation
   --------------------------------

NOTE: If you do not have OS/2 2.1+, contact IBM and request OS/2 2.1+
      (beta or release).  The following assumes you are installing
      OS/2 2.1+.

The following steps are required to add OS/2 2.1 support for the HT216
family of SVGA controllers.  These steps assume the HT216 distribution
disk is in drive A and OS/2 is on drive C.

1) Install OS/2 2.1 normally.

2) Create the HEADLAND subdirectory.
	a. Open a DOS window.
	b. Type "md os2\headland".

3) Unzip the HT216 OS/2 support files.
	a. Type "A:".
	b. Type "pkunzip os2_2x c:\os2\headland".

4) Rename SVGA.EXE.
	a. Type "C:".
	b. Type "cd \os2".
	c. Type "rename SVGA.EXE SVGA_IBM.EXE"
	d. Type "copy headland\SVGA.EXE".

5) Rename VSVGA.SYS
	a. Type "cd mdos".
	b. Type "rename "VSVGA.SYS VSVGAIBM.SYS".
	c. Type "copy ..\headland\VSVGA.SYS".
	d. Type "exit".

6) Update CONFIG.SYS using "OS/2 System Editor
	a. Open the file C:\CONFIG.SYS with OS/2 System Editor.
	b. Find the line that starts with "LIBPATH=.;C:\..."
	c. Modify this line to include the HEADLAND subdirectory.
		"LIBPATH=C:\OS2\HEADLAND;.;C:\..."
	d. Save the changed file.

7) Restart OS/2.

8) Change display resolution.
	a.  Start "Selective Install" from the System Startup folder.
	b.  Select "Super Video Graphics Array" for Primary display
		if it is not already chosen.
	c.  Select "OK" button.
	d.  Select "INSTALL" button.
	e.  After a few minutes of processing, a dialog box will appear
		with a choice of display resolutions.  Choose one.

9) Restart OS/2.  Your new resolution will be in use.


   IBM OS/2 1.X Installation
   -------------------------

Please follow directions in IBM OS/2 1.X manual.



