Firmware Update Guide

1. DOS
	boot to dos, and run dosfls

2. Linux
	boot to Linux and execute "./linuxfls"
	As  uh8l have its own IPMI driver, beforing flashing,
	make sure no other IPMI driver loaded.