970A-G45 /970A-G46 (MS-7693) V2.8 BIOS Release
-------------------------------------------------

1. This is AMI BIOS release

2. This BIOS fixes the following problem of the previous version:
-  Unlock function will be failed with some particular cpu.

3. 2016/01/08

----------------------------------------------------------------------------------------
Note:
* Please download and execute the file in USB pen drive only.
  System will restart several times to update system BIOS with NVRAM & ROMHOLE.
  Please DO NOT remove the USB pen drive until BIOS updated successfully.
* Please make sure you have read the SOP before you update the BIOS.
* MSI recommend you to update BIOS only if you are using Windows8.
* There is no way to reflash back to BIOS version 1xx if you already updated to version 2xx.
-----------------------------------------------------------------------------------------

[Below information is Chinese language]

A. AMI BIOS 正式發行

B. 此版本修正下列問題:
-  搭配使用一些CPU時, 開核功能有時會失敗.

C. 更新日期: 公元2016年01月08號

----------------------------------------------------------------------------------------------------------
備註:
* 請務必將檔案下載於 USB 隨身碟中.並在 USB 隨身碟中執行.
  系統在更新完 BIOS 之後, 將會重啟幾次準備更新 NVRAM 及 ROMHOLE, 在未確認更新完成之前, 請勿移除 USB 隨身碟.
* 請在更新 BIOS 前, 務必先詳讀作業指導書.
* 如果您並非安裝 Windows8, 建議您不需更新主機板韌體版本至 v.2xx.
* 主機板韌體版本在更新至 v.2xx 之後, 將無法回到版本 v.1xx.
-----------------------------------------------------------------------------------------------------------
