BIOS History For Foxconn
==============================================================================
Model :	P55A01 GTI		FAB : 1.0		Author : Arcer Hwang
Old version : 97AF1D01.BIN, 97AF1D01.ROM
New version : 97AF1D02.BIN(2MB)	Code Base : 02/20/2009	Build date : 08/12/2009
New version : 97AF1D02.ROM(1MB)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : FD00(h) 97AF1D02.BIN
CheckSum  : 9C8E(h) 97AF1D02.ROM
Description for Customer :
	1. Fixed recovery card issue.
	2. Fixed sometime hang-up at BIOS POST code D3h.
	3. Fixed memory size show wrong with Clarkdale CPU.
==============================================================================
Model :	P55A01 GTI		FAB : 1.0		Author : Arcer Hwang
Old version : 97AF1D02.BIN, 97AF1D02.ROM
New version : 97AF1P01.BIN(2MB)	Code Base : 02/20/2009	Build date : 08/12/2009
New version : 97AF1P01.ROM(1MB)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 7F9E(h) 97AF1P01.BIN
CheckSum  : 1F37(h) 97AF1P01.ROM
Description for Customer :
	1. First release P version.
==============================================================================
Model :	P55A01 GTI		FAB : 1.0		Author : Arcer Hwang
Old version : 97AF1P01.BIN, 97AF1P01.ROM
New version : 97AF1D03.BIN(2MB)	Code Base : 02/20/2009	Build date : 08/13/2009
New version : 97AF1D03.ROM(1MB)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : F8F7(h) 97AF1D03.BIN
CheckSum  : 9890(h) 97AF1D03.ROM
Description for Customer :
	1. Modify USB initialization field value(EDS SU 1.54).
==============================================================================
Model :	P55A01 GTI		FAB : 1.0		Author : Arcer Hwang
Old version : 97AF1D03.BIN, 97AF1D03.ROM
New version : 97AF1D04.BIN(2MB)	Code Base : 02/20/2009	Build date : 08/21/2009
New version : 97AF1D04.ROM(1MB)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : AD02(h) 97AF1D04.BIN
CheckSum  : 4C9B(h) 97AF1D04.ROM
Description for Customer :
	1. Update AMI BIOS Piketon platform NB code to version 024.
	2. Update AMI BIOS Piketon platform PCH code to version 030.
	3. Update AMI BIOS Intel PPM DT code to version 02.00.
	4. Update Intel Lynnfield and Clarkdale CPU microcode as bellow :
	   M13106E5_00000003.TXT,M1320651_FFFF000F.TXT,M1320652_FFFF0008.TXT.
	5. Added Support OC Recovery feature.
==============================================================================
Model :	P55A01 GTI		FAB : 1.0		Author : Arcer Hwang
Old version : 97AF1D04.BIN, 97AF1D04.ROM
New version : 97AF1P02.BIN(2MB)	Code Base : 02/20/2009	Build date : 09/03/2009
New version : 97AF1P02.ROM(1MB)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 912D(h) 97AF1P02.BIN
CheckSum  : 30C6(h) 97AF1P02.ROM
Description for Customer :
	1. Removed DMI type 3 information.
	2. Modify DMI Slot information.
==============================================================================
Model :	P55A01 GTI		FAB : 1.0		Author : Arcer Hwang
Old version : 97AF1P02.BIN, 97AF1P02.ROM
New version : 97AF1P03.BIN(2MB)	Code Base : 02/20/2009	Build date : 09/17/2009
New version : 97AF1P03.ROM(1MB)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 4E0F(h) 97AF1P03.BIN
CheckSum  : EDA8(h) 97AF1P03.ROM
Description for Customer :
	1. Modify BIOS for WLK 1.4.
==============================================================================
Model :	P55A01 GTI		FAB : 1.0		Author : Arcer Hwang
Old version : 97AF1P03.BIN, 97AF1P03.ROM
New version : 97AF1P04.BIN(2MB for factory)	Code Base : 02/20/2009	Build date : 10/30/2009
New version : 97AF1P04.ROM(1MB for update BIOS utility FPT.EXE or FPTW.EXE)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 4C62(h) 97AF1P04.BIN
CheckSum  : EBFB(h) 97AF1P04.ROM
Description for Customer :
	1. Update BIOS code for support Clarkdale C2 steping CPU(CPUID:20652).
==============================================================================
Model :	P55A01 GTI		FAB : 1.0		Author : Arcer Hwang
Old version : 97AF1P04.BIN, 97AF1P04.ROM
New version : 97AF1P05.BIN(2MB for factory)	Code Base : 02/20/2009	Build date : 11/25/2009
New version : 97AF1P05.ROM(1MB for update BIOS utility FPT.EXE or FPTW.EXE)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : C69A(h) 97AF1P05.BIN
CheckSum  : 6633(h) 97AF1P05.ROM
Description for Customer :
	1. Fixed Lynnfield 750 CPU(CPUID:106E5) show wrong core count.
	2. Fixed Clarkdale G9650 CPU(CPUID:20652) hang-up on BIOS CMOS setup CPU Configuration page.
	3. Fixed dale CPU PEG port can't run link x16 mode.
==============================================================================
Model :	P55A01 GTI		FAB : 1.0		Author : Arcer Hwang
Old version : 97AF1P05.BIN, 97AF1P05.ROM
New version : 97AH6S01.BIN(2MB for factory)	Code Base : 02/20/2009	Build date : 01/21/2010
New version : 97AH6S01.ROM(1MB for update BIOS utility FPT.EXE or FPTW.EXE)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 4027(h) 97AH6S01.BIN
CheckSum  : 9D65(h) 97AH6S01.ROM
Description for Customer :
	1. Fixed USB port can't connect to iPhone.
	2. Added SLP21 and logo for customer Hi-Grade(logo file : Hi-Grade.jpg)
	3. Update Ignition firmware from version 6.0.0.1126 to version 6.0.30.1199 for 97AH6S01.BIN.
==============================================================================
Model :	P55A01 GTI		FAB : 1.0		Author : Arcer Hwang
Old version : 97AF1P05.BIN, 97AF1P05.ROM
New version : 97AF1P06.BIN(2MB for factory)	Code Base : 02/20/2009	Build date : 04/09/2010
New version : 97AF1P06.ROM(1MB for update BIOS utility FPT.EXE or FPTW.EXE)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 91B2(h) 97AF1P06.BIN
CheckSum  : EEF0(h) 97AF1P06.ROM
Description for Customer :
	1. Fixed USB port can't connect to iPhone.
	2. Update Ignition firmware from version 6.0.0.1126 to version 6.0.30.1199.
	3. Added support CPU i7-875K(Q3Z3),i5-655K(Q4MA),i7-880(Q3M5),i7-870S(Q3MT),i3-550(Q4DD).
==============================================================================
Model :	P55A01 GTI		FAB : 1.0		Author : Arcer Hwang
Old version : 97AF1P06.BIN, 97AF1P06.ROM
New version : 97AF1P07.BIN(2MB for factory)	Code Base : 02/20/2009	Build date : 05/11/2010
New version : 97AF1P07.ROM(1MB for update BIOS utility FPT.EXE or FPTW.EXE)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 0D56(h) 97AF1P07.BIN
CheckSum  : 6A94(h) 97AF1P07.ROM
Description for Customer :
	1. Fixed CPU i7-875K(Q3Z3),i5-655K(Q4MA) OS blue screen issue.
	2. Update CPU microcode for CPUID 106E5(M13106E5_00000004.TXT).
==============================================================================