AMI ROM Tool - AFUWIN

Description :
	AMI Firmware Update utility(APTIO) for pure 64bits WINDOWS.

Release Date :


Source Control Location :
	SS: Alaska;$/Alaska/ROMUtils/AFU/afuwin/64;

Reference Document :	
	readme.txt
	readme_afuwin.txt
	AMI_Aptio_AFU_User_Guide_NDA.pdf

Known Issues :
    Use "/Rn" parameter will have no effect or caused an exception error, when 
    the SMBIOS module version is between "4.6.1_ALPHA_01.26.2_DMIRW_TEST" and 
    "(INT)4.6.1_ALPHA_01.29_Type39".

Release Notes:
==============================================================================
3.02
	01.Support get smi port number from ACPI table.
	02.Support new secure ROM file image Get capsule header when exist inside in ROM file.
	03.Support new secure Rom file image Update /ME use the same file.
	04.Support OFBD default configure for /capsule, /recovery /OA /OAD.
	05.Support AFUWINGUI.
	06.Support /A the same and not the same error message.
	07.Fix Error message. When secure mode not support use /capsule or /recovery will show "unknow command".
	08.Fix Error message. When secure mode not support use command will show 0x15 error message.
	09.Fix DMI Data Preserve fail. When DMI Data report size not match.
	10.Fix DMI Data Preserve fail. When rom block size is 4k.
	11.Fix DMI Data Preserve fail. When DMI data in NVRAM and use command /b /n /r .
	12.Fix EC update fail. When Secure mode support and use command /e and /capsule or /recovery.
	13.Fix EC update fail. When Secure mode support and use only /e command.
	14.Fix MER update fail.
	15.Fix open fail file error.
==============================================================================
3.01
	01. Migrate features from AMIAFUAPTIO v2.39
	02. Support Secure Flash /P /B /N preserving Romholes and OA Key.
	03. Support OA 3.0 Microsoft requirements. [EIP 77891][EIP 77107]
	04. Support /Kn option for updating non-critical blocks with .bin files.
	05. Support /L /Ln options for updating Romhole data. /K /Kn options are now used for 
	    updating non-critical blocks only.
	06. Fix Windows 64bit OS driver.
	07. Fix write-protected function fail issue.[EIP 80549]
	08. Fix /A option flashing over existing MDSM data.[EIP 82266]
	09. Fix issue of not preserving SMIBIOS data.
	10. Fix issue of unrecognizing two-FV Romhole.
	11. Fix error message in AFUWINx64.

==============================================================================
3.00
	01. Migrate features from AMIAFUAPTIO AFUWIN 2.38
	02. Supports Security Flash module and adds two new options: /CAPSULE and /RECOVERY for
	    overriding Secure Flash policy by capsule or recovery.
	03. Supports deleting OEM Activation Key [/OAD].