This BIOS is for the EVGA Z77 Stinger motherboard.

This package contains the necessary Flash Tool and binary file to Flash your EVGA Motherboard. Please check to ensure 
that you downloaded the right package for your motherboard.


This flash is designed for Windows 32Bit/64Bit or DOS mode.

    * First go into your BIOS and load defaults, save and exit
    * Go into the folder where you unzipped this package and run the appropriate batch file.
          o For Windows XP, Vista or 7 32Bit: fptwin32.bat
          o For Windows XP, Vista or 7 64Bit: fptwin64.bat
          o If in DOS Mode: FPTDOS.BAT 
    * Press Y in CAPITAL LETTERS to start the flash process
    * DO NOT TURN OFF POWER OR RESET DURING THE FLASH PROCESS
    * After the flashing is finished, the system will shut down. Then power on again and go into BIOS, Load Defaults, Save and Exit. 


Warning:
**Do not restart or interrupt your PC while the flash is ongoing
**Do not Flash BIOS on overclocked settings
**It is always recommended to power-down after flash