If you want to update your BIOS, please execute the BAT file. Don't use awdflash/AFUDOS directly.
When you execute the BAT file, it will automatic run the flash utility to update the new BIOS for your mainboard.(Note: Before update BIOS please make sure already disabled Flash Part Protect function in BIOS Setup)
The new BIOS was modified for the following reason:
    1.Update USB Code.Support USB HUB.(AMI)
    2.Fix USB KeyBoard/Mouse can't work under DOS.(AMI)
    3.Fix system is unstable with Nvidia Geforce 2 series VGA card.(AMI)
    4.Modify clockgen code for system stability.(AMI)
