If you want to update your BIOS, please execute the BAT file. Don't use AFUDOS/AwdFlash directly.
When you execute the BAT file, it will automatic run the flash utility to update the new BIOS for your mainboard.(Note: Before update BIOS please make sure already disabled Flash Part Protect function in BIOS Setup)
The new BIOS was modified for the following reason:
    1.Update AgesaCode to 3.7.1.2(AMI).
    2.Fix no display sometimes if use NVIDIA Geforce GT 4XX VGA card.(AMI)
    3.Support ALC887.(AMI)

