
18MLCD.ROM      This BIOS support MONO DSTN 640*480 LCD panel. It can
                drive following panel:
                     (1) HOSIDEN HLM6667
                     (2) HITACHI LMG5160XUFC
                     (3) CASIO MD650TS00-01
                     (4) OPTREX DMF_50260NFU-FW-8

18DSTN.ROM      This BIOS support Color DSTN 640*480 LCD panel. It can
                drive following panel
                     (1) Sanyo LCM-5331-22NTK
                     (2) SHARP LM64C35P

18TFTs1.ROM     This BIOS support TFT 640*480-Sync 16 BIT panel.

18TFTs2.ROM     This BIOS support TFT 640*480-Sync 18/24 BIT panel. It can
                drive following panel:
                     (1) HITACHI TX26D60/TX24D55
                     (2) TOSHIBA LTM09C015A,LTM10C209A
                     (3) SHARP LQ10D321
	
18TFTLP1.ROM    This BIOS support TFT 640*480-LP 16 BIT panel.

18TFTLP2.ROM    This BIOS support TFT 640*480-LP 18/24 BIT panel. It can
                drive
                     Toshiba LTM09c015A panel.

18TFT861.ROM    This BIOS support TFT 800*600_sync 16 BIT panel.

18TFT862.ROM    This BIOS support TFT 800*600_sync 18/24 BIT panel. It can
                drive following panel:
                     (1) NEC NL8060AC26-05
                     (2) NEC NL8060AC26-04
                     (3) NEC NL8060BC31-02

18EL.ROM        This BIOSsupport EL 640*480 panel. It can drive
                     PLANAR EL640.480-A panel.

18PLASMA.ROM    This BIOS support PLASMA 640*480 panel. It can drive
                     PANASONIC S817 panel.

18CRT.ROM       This BIOS support CRT only.

