Intel G41 chipset (G41 + ICH7, LGA775, DDR-III) mATX

AMI BIOS


I0819FZT.ROM  	BIOS for (G41+ ICH7,  Fintek Super IO) 
		*** with Hardware Monitor 
		*** with STR (Suspend-To-RAM)
		*** with on-board LAN
		*** with 6-Ch HD Audio
		*** with Zotac Full Screen Logo


.8Mbit Flash size
.Initial mass production release
(Aug / 2009)

.8Mbit Flash size
.Fixed DDR3 RAM (Single Side  2GB / 4GB Module) compatibility issue
.Fixed POST screen wrong HDD size
(Nov / 2010)

.8Mbit Flash size
.Changed DMI content for "ZOTAC"
(Nov / 2010)

.8Mbit Flash size
.2011/June built
.Special for Audio Codec ALC887

.8Mbit Flash size
.2011/Aug update built
.Supported both Audio Codec ALC662 and ALC887
.Fixed built-in graphic screen stability issue
(Aug / 2011)