AMI ROM Tool - AFUWIN

Description :
	AMI Firmware Update utility(APTIO) for pure 64bits WINDOWS.

Release Date :


Source Control Location :
	SS: AptioV;$/AptioV/RomUtils/Afu/AfuWin/64;

Reference Document :	
	readme.txt
	readme_afuwin.txt
	AMI_AptioV_AFU_User_Guide_NDA.pdf

Known Issues :
    Use "/Rn" parameter will have no effect or caused an exception error, when 
    the SMBIOS module version is between "4.6.1_ALPHA_01.26.2_DMIRW_TEST" and 
    "(INT)4.6.1_ALPHA_01.29_Type39".

Release Notes:
==============================================================================
5.06.00
	[AFU]
	1.Fix ECX erase szie issue.[EIP105071]
	2.Fix UCP insert ROM file AFU can't open issue.
	3.Fix command /OAD can't flash issue, when secure flash enable.
	4.Fix, AFU can't find FID OA key issue, when ROM data have many _FVH string.
	5.Fix When NVRAM is full, and SMIBIOS data in NVRAM, AFU can't preserve this data.
	6.Fix When flash /p /b /n add /me command, AFU will not preserve need preserve data.
	7.Fix When ROM Hole size exceed two block size, /holeout bin file is not right data.
	8.Fix When new rom Rom Hole offset different old rom rom hole offset, use /p /b /n /ln, 
	  ln rom hole data will be update to old rom offset.[EIP157284]
	9.Modify Copright to 2014.
	10.Modify when use command /ln, AFU check platform have not rom hole, AFU will show,
	   "Error: Rom Hole not exist."

	[Error Message Change]
	1."Error: OA Data invalid." to "Error: OA key data is invalid."
	2."Error: OA key is not NULL at all. And OA Key is the same as Bin File in system." to 
	  "Error: OA key is not empty at all. And OA Key is the same as Bin File in system."
	3."Error: OA key is NULL at all already." to "Error: OA key is empty at all already."
	4."Error: OA key is not NULL at all. And OA Key is no the same as Bin File in system." to 
	  "Error: OA key is not empty at all. And OA Key is no the same as Bin File in system."
	5."Error: Unable to start a Secure Flash session." to "Error: Secure Flash Rom Verify fail."
==============================================================================
5.05.04
	[AFU]
	1.Fix SMBIOS Data can't restore, when SMBIOS Data in NVRAM and NVRAM is full. [EIP145538],[EIP145305]
==============================================================================
5.05.03
	[AFU]
	1.Change Version 3.05.02 to 5.05.03.
	2.Fix check EC bin file header data return result error.
	3.Fix Rom Hole does not Alignment block error.[EIP143348]

	[AFUGUI-MFC]
	1.Fix WINGUI Show OFBD ROM ID Check dialog issue.[ECR191374]
	2.Fix WINGUI Show OFBD EC dialog issue.
