;============================
; W888 BIOS Information:
; 
; Base Address:
; RCBA:
; MCHBAR:
; Real-Time Ratio Control:
;
; Port 1      - LAN2        ... PCI Express LAN 2
; Port 2      - 1394B       ... 1394 Net Adapter
; Port 3      - LAN1        ... PCI Express LAN 1
; Port 4      - USB3_HOST3  ... USB 3.0 (port 2/3)
; Port 5(x2)  - SATA3       ... E-SATA  (PCIe x2)
; Port 6(dis) - 
; Port 7      - USB3_HOST2  ... USB 3.0 (port 4/5)
; Port 8      - USB3_HOST1  ... USB 3.0 (port 0/1)
;=====================================================================================================================================

R000 11/28/2011
	R000    EVGA BIOS format adjustment.
	R000_1	Non-support "Built-in Shell".
	R000_2  Non-support "F71889_FLOPPY_PORT".
	R000_3  Non-support "F71889_PARALLEL_PORT".
	R000_4  Non-support "F71889_SERIAL_PORT1".
	R000_5  Non-support "F71889_SERIAL_PORT2".
	R000_6  Default set "QUIET_BOOT", "FORCE_USER_TO_SETUP_ON_FIRST_BOOT" enabled.
	R000_7  Default set "CLEAR_PS2KB_BUFFER_AT_READYTOBOOT" enabled.
	R000_8  Default set "100 x 31 terminal resolution" enabled (fix BIOS screen narrow down.)
	R000_9  Default set "Port 60/64 Emulation" disabled.
	R000_10 Default set "End of Post Message" disabled.
	R000_11 Default set "IOU2/IOU3 PCIe Port" from x8x8 to x16.
	R000_12 Add/Move following itmes satisfied EVGA BIOS Setup, that.
		a. "USB Port 0 ~ 9" & "BlueTooth"	(Chipset      -> Advanced ).
		b. "SATA Port 0 ~ 5" position		(South Bridge -> Advanced ).
		c. "PXE OpROM, Storage OpROM"		(Advance      -> Chipset  ).
		d. "Restore AC Power Loss"		(South Bridge -> Chipset  ).
		e. "On-Board Device Group creating"
		f. "PCI Express Port 0 ~ 8"		(South Bridge -> On-board Device ).
		g. "Azalia HDAudio".			(South Bridge -> On-board Device ).
		h. "High Precision Event Timer"		(South Bridge -> On-board Device ).
		i. "CPU Configuration"			(Advanced     -> OverClocking    ).

	R000_13 Hide "Access Level"
	R000_14 Hide "Save Options"
	R000_15 Hide "XHCI Hand-off"
	R000_16 Hide "EHCI Hand-off"
	R000_17 Hide "Network Stack"
	R000_18 Hide "USB3.0 Support"
	R000_19 Hide "AMT Configuration"
	R000_21 Hide "Trusted Computing"
	R000_22 Hide "WHEA Configuratison"
	R000_23 Hide "Straggered Spin-up"
	R000_24 Hide "Port 60/64 Emulation"
	R000_25 Hide "USB transfer time-out"
	R000_26 Hide "Device reset time-out"
	R000_27 Hide "Device power-up delay"
	R000_28 Hide "AMI Debug Rx Enabled!"
	R000_29 Hide "Runtime Error Logging"
	R000_30 Hide "Thermal Configuration"
	R000_31 Hide "Lock Legacy Resources"
	R000_32 Hide "Save as User Defaults"
	R000_33 Hide "Restore User Defaults"
	R000_34 Hide "PCI Subsystem Settings"
	R000_35 Hide "Super IO Configuration"
	R000_36 Hide "Chipset Reference Board"
	R000_37 Hide "External SATA Port 0 ~ 5"
	R000_38 Hide "USB HW delays and time-outs:"
	R000_39 Hide "Serial Port Console Redirection"
	R000_40 Hide "DYNAMIC_PAGES(Port Configuration)"
	R000_41 Hide "Launch EFI Shell from filesystem device"
	R000_42 Hide "CSM Support"
	R000_43 Hide "North Bridge"
	R000_44 Hide "South Bridge"
	R000_45 Show "SAS Port 4 ~7" whether CPU1 installed or not.
	R000_46 Rename "Port 0 ~5 Hot Plug" to " Hot Plug"
	R000_47 Rename "ACPI Setting" to "ACPI configuration"
	R000_48 Rename "Project Version" to "BIOS Version"

	R000_55 Update DMI String for EVGA Information.
	R000_56 Support "SLi function"
	R000_57 Support "USB Beep Optional"
	R000_58 Support "Cear CMOS function"
	R000_59 Support "USB3.0 Host Controller boot"
	R000_60 Support "PWRBTN LED color control in S3"
	R000_61 Support "S3 execution with S4 disabled in BIOS Setup"
	R000_62 Support "CPU Temperature Monitor" (CPU Temp shows on 80 port).


R001 12/16/2011
	R001_1  Update HDAudio Verb Table.
	R001_2  Grayout PCIe port 1 with enabled.
	R001_3  Fixed "LAN2 not functional after disable LAN1 in BIOS Setup". (Bug#371)
	R001_4  Fixed "USB2.0 ports can't detect USB Drive & USB HDD".        (Bug#357)


R002 12/29/2011
	R002_1  Support "Sandy Bridge-EP C2 CPU" (update microcode 028 -> 033).
	R002_2  Support "PS/2 Mouse"          (Bug#212)
	R002_3  Support "Setup Profile"       (Bug#381)
	R002_4  Fixed "S/PDIF-IN no function" (Bug#367)
	R002_5  Fixed "Execute S3 will automatically wake up system" (Bug#353)


R003 01/06/2012
	R003_1  Update SMBIOS System Information.   (Bug#382)
	R003_2  Fixed "LAN2 S4 Wake on LAN failure" (Bug#395)
	R003_3  Add "DIMM Configuration" to OverClocking.


R004 01/18/2012
	R004_1  HW Monitor Implementation. (Bug#375)


R005 02/03/2012
	R005_1  Update formal POST LOGO.
	R005_2  Add "IOH Configuration" into Chipset Menu.
	R005_3  Support "Turbo Mode" with default setting.
	R005_4  Fixed "Restore AC power loss fail" (Bug#379).


R006 02/23/2012
	R006_1  Update AMI codebase to vesion 015.
	R006_2  Update PXE OpROM to formal ver1.3.81           (Bug#376)
	R006_3  Add "SAS OpROM" item.
	R006_4  Support "iOne Scorpius-U9GBL USB KB"           (Bug#340)
	R006_5  Fixed "CPU occurs yellow band in WinXP 64-bit" (Bug#387)


R007 03/15/2012
	R007_1  Add "Voltage adjustment items".
	R007_2  Update onboard device text for H/W Rev1.0. (USB port, USB Header & SAS)


R008 03/21/2012
	R008_1  Fix "SAS HDD can't be detected". (Bug#374, Bug#378, Bug#383)
	R008_2  Fix "AUX_FAN not show speed".
	R008_3  Update ME Firmware to ver. 7.1.40.1161


R009 03/23/2012
	R009_1  Fix "SAS HDD Installation failure"


R010 03/30/2012
	R010_1  Add "IOU 2 VGA card auto detection"
	R010_3  Add "Memory XMP"


R011 04/13/2012
	R011_1  Light up NumLock while enter BIOS Setup.
	R011_2  Support "System Fan(CHA_FAN1, SYS_FAN1, SYS_FAN2) with 2 CPU".
	R011_3  Support "ERP Power Saving Function".
	R011_4  Remove solution R009_1.


R012 04/27/2012
	R012_1  Fix "BCLK>103MHz will crash system".
	R012_2  Fix "Install UEFI OS to SAS HDD will crash".


R013 05/18/2012
	R013_1  Fix "S3 resume will crash at second times".
	R013_2  Fix "Voltage(Dimm5/6/7/8, P0_VSA, CPU_PLL) show error value"
	R013_3  Fix "tRFC value error with different memory speed"


R014 06/14/2012
	R014_1  Update microcode version from 034 to 039.
	R014_2  Support "PS/2 KB, Mouse wake up from S3 and S4 state".
	R014_3  Support "Memory Timings control with 2 CPU".
	R014_4  Update "PXE Option Rom" to fix error message.


R015 06/22/2012
	R015_1  Support GTX-690/GTX-590(dual GPU card).
	R015_2  Fix "Install new nVIDIA driver will occur blue screen(0x00000122)"
	R015_3  Update ME version from 7.1.40.1161 to 7.1.52.1176
	R015_4  Support Corsair K60 Keyboard.


R016 09/18/2012
	R016_1  Support "ECC 1600 1.35V RDIMMs"


R017 12/28/2012
	R017_1  Reserve PCI resource(e-SATA disabled) to support Qio storage card.


R018 03/05/2013
	R018_1  Support nVIDIA Titan & Quadro VGA card.


R019 03/06/2013
	R019_1  Fix "In Raid Mode, Boot Manger(F7) not list HDD devices."


R020 03/20/2013
	R020_1  Fix "SAS device can't be detected".