If you want to update your BIOS, please execute the BAT file. Don't use awdflash/AFUDOS   directly.
When you execute the BAT file, it will automatic run the flash utility to update the new BIOS for your mainboard.(Note: Before update BIOS please make sure already disabled Flash Part Protect function in BIOS Setup)
The new BIOS was modified for the following reason:
    1.First release for production.(AMI BIOS)
    2.Update AgesaCode to 3.3.2.3.(AWARD BIOS)
    3.Fix system hung up when use winflash to update BIOS.(AWARD BIOS)
