If you want to update your BIOS, please execute the BAT file. Don't use awdflash/AFUDOS directly.
When you execute the BAT file, it will automatic run the flash utility to update the new BIOS for your mainboard.(Note: Before update BIOS please make sure already disabled Flash Part Protect function in BIOS Setup)
The new BIOS was modified for the following reason:
    1. Update Northbridge CIM Code.(AWARD BIOS)
    2. Fix sometimes HD3850 VGA card no display.(AWARD BIOS)
    3. Update PXE ROM to 2.28.(AWARD BIOS)
