If you want to update your BIOS, please execute the BAT file. Don't use awdflash/AFUDOS directly.
When you execute the BAT file, it will automatic run the awdflash/AFUDOS to update the new BIOS for your mainboard.(Note: Before update BIOS please make sure already disabled Flash Part Protect function in BIOS Setup)
The new BIOS was modified for the following reason:
	AWARD BIOS:
 		1£®Update PXE ROM to v2.30
		2 .  Add watch dog to solve sideport can't use normally in low temp 
        AMI BIOS:
                1£®Update CPU code to AGESA 3.3.2.7
		2£®Update PXE ROM to v2.30
		3 .  Add watch dog to solve sideport can't use normally in low temp 
		4 .  add flash protect function



  