Note:	before start, it is better to remove all bootable devices like SATA HDD.
	Otherwise you may need to change to different drive label (fs1, fs2...etc) instead of fs0: in step 3

1. Put BIOS in USB drive, and then attach USB drive to system.
2. Select boot for Built-in Shell (or shell loader in USB drive if present. You can find it in BIOS Setup Boot page).
3. Move operating directory to USB drive (fs0 or other labels) by entering "fs0:" (Type "fs0:" then press Enter key)
   > fs0:
4. Enter the directory with BIOS file and update batch (The directory that you put the BIOS image)
5. Execute update batch (go_x64.nsh)
6. Confirm update procedure is passed without problem
7. Reboot system