Prepare Bootable USB
1] Format USB using command > format /FS:FAT /Q <THUMB DRIVE LETTER>:
2] Run Command > vxysysNT.exe <THUMB DRIVE LETTER>:
3] Copy bootrom.bin/bootrom.sys to USB Thumb drive using copy command line only.
3] Copy vxWorks.st to USB Thumb drive using copy command line only.